B E I P R S T V W

## P

PL2303Device_GetCommTimeouts(int) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  The PL2303Device_GetCommTimeouts retrieves the time-out parameters for all read and write operations on a specified communications device.
PL2303Device_GetSerialNumber() - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Get PL2303G serial number.
PL2303Device_IsHasPermission() - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Detecting whether this PL2303 devices has permission.
PL2303Device_IsSupportChip() - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Detecting whether this PL2303 supports this Android OS, only PL2303G is supported.
PL2303Device_SetCommTimeouts(int) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  The PL2303Device_SetCommTimeouts function sets the time-out parameters for all read and write operations on a specified communications device.
PL2303G_CTS_ON - Static variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
PL2303G_DCD_ON - Static variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
PL2303G_DSR_ON - Static variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
PL2303G_Enable_GPIO_A(int, boolean) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to control the direction of these pins GPIO_A.
PL2303G_Enable_GPIO_B(int, boolean) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to control the direction of these pins GPIO_B.
PL2303G_Get_GPIO_Value_A(int) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  PL2303G has 8 software controllable, General-purpose input and output control signal pins.
PL2303G_Get_GPIO_Value_B(int) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  PL2303G has 8 software controllable, General-purpose input and output control signal pins.
PL2303G_GPIO_A_CNT_ENABLE(int, boolean) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to Init GPIO_A.
PL2303G_GPIO_B_CNT_ENABLE(int, boolean) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to Init GPIO_B.
PL2303G_RI_ON - Static variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
PL2303G_Set_GPIO_Value_A(int, int) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  PL2303G has 8 software controllable, General-purpose input and output control signal pins.
PL2303G_Set_GPIO_Value_B(int, int) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  PL2303G has 8 software controllable, General-purpose input and output control signal pins.
PL2303GDriver<UsbConfiguration> - Class in tw.com.prolific.driver.pl2303g
PL2303GDriver(UsbManager, Context, String) - Constructor for class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Initialize a PL2303G driver, the software 4K Queue buffer is enable.
PL2303GDriver(UsbManager, Context, String, boolean) - Constructor for class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Initialize a PL2303G driver.
PL2303GDriver.BaudRate - Enum in tw.com.prolific.driver.pl2303g
PL2303GDriver.DataBits - Enum in tw.com.prolific.driver.pl2303g
PL2303GDriver.FlowControl - Enum in tw.com.prolific.driver.pl2303g
PL2303GDriver.Parity - Enum in tw.com.prolific.driver.pl2303g
PL2303GDriver.StopBits - Enum in tw.com.prolific.driver.pl2303g
PL2303LibGetVersion(byte[]) - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Get the version of this library.
PL2303USBFeatureSupported() - Method in class tw.com.prolific.driver.pl2303g.PL2303GDriver
  Detecting whether this Android OS supports USB host API feature.
PL_MAX_INTERFACE_NUM - Static variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
PLDETACHED_VALUE - Variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
PLUART_DETACHED - Variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver
PLUART_MESSAGE - Variable in class tw.com.prolific.driver.pl2303g.PL2303GDriver

B E I P R S T V W