B E P T V

## P

PL2303CloseDeviceByIndex(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Close an PL-UART USB Device by index.
PL2303Device_GetCommTimeouts(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  The PL2303Device_GetCommTimeouts function retrieves the time-out parameters for all read and write operations on a specified communications device.
PL2303Device_GetSerialNumber(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
PL2303Device_SetCommTimeouts(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  The PL2303Device_SetCommTimeouts function sets the time-out parameters,
  for all read and write operations on a specified communications device.
PL2303Enumerate() - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Found a PL2303G device number , the default VID_PID is 067B_2303.
PL2303G_CTS_ON - Static variable in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
PL2303G_DCD_ON - Static variable in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
PL2303G_DSR_ON - Static variable in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
PL2303G_Enable_GPIO_A(int, int, boolean) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to control the direction of these pins GPIO_A.
PL2303G_Enable_GPIO_B(int, int, boolean) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to control the direction of these pins GPIO_B.
PL2303G_Get_GPIO_Value_A(int, int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to get the status of these GPIO_A pins when the direction is in input mode.
PL2303G_Get_GPIO_Value_B(int, int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to get the status of these GPIO_B pins when the direction is in input mode.
PL2303G_GPIO_A_CNT_ENABLE(int, int, boolean) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to Init GPIO_A.
PL2303G_GPIO_B_CNT_ENABLE(int, int, boolean) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to Init GPIO_B.
PL2303G_ReSetStatus() - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  ReSet Port Status.
PL2303G_RI_ON - Static variable in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
PL2303G_Set_GPIO_Value_A(int, int, int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to control the status of these pins of GPIO_A when the direction is output mode.
PL2303G_Set_GPIO_Value_B(int, int, int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  PL2303G has 8 software controllable, General-purpose input and output control signal pins,
  You can use this API to control the status of these pins of GPIO_B when the direction is output mode.
PL2303G_SetDTR(int, boolean) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Switch PL2303G DTR on or off.
PL2303G_SetRTS(int, boolean) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Switch PL2303G RTS on or off.
PL2303getCOMNumber(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Get the PL2303G COM port Number : COM1, COM2, COM3...
PL2303getDevicePathByIndex(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Get the Device Path.
PL2303getProlificUSBDeviceCount() - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Returns the active device number of PL2303.
PL2303getSerialByIndex(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Returns the serial number for the device.
PL2303GMultiLib - Class in tw.com.prolific.pl2303gmultilib
PL2303GMultiLib(UsbManager, Context, String) - Constructor for class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Initialize a PL2303G driver, the software 4K Queue buffer is enable.
PL2303GMultiLib(UsbManager, Context, String, boolean) - Constructor for class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Initialize a PL2303G driver.
PL2303GMultiLib.BaudRate - Enum in tw.com.prolific.pl2303gmultilib
PL2303GMultiLib.DataBits - Enum in tw.com.prolific.pl2303gmultilib
PL2303GMultiLib.FlowControl - Enum in tw.com.prolific.pl2303gmultilib
PL2303GMultiLib.Parity - Enum in tw.com.prolific.pl2303gmultilib
PL2303GMultiLib.StopBits - Enum in tw.com.prolific.pl2303gmultilib
PL2303IsDeviceConnectedByIndex(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Get the connection status of this PL2303G, ie, whether there is an active connection with PL2303G device.
PL2303LibGetVersion(byte[]) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Get Lib version.
PL2303OpenDevByBaudRate(int, PL2303GMultiLib.BaudRate) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Open an PL-UART USB Device by baudrate.
PL2303OpenDevByDefualtSetting(int) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Open an PL-UART USB Device by default UART setting.
PL2303OpenDevByUARTSetting(int, PL2303GMultiLib.BaudRate, PL2303GMultiLib.DataBits, PL2303GMultiLib.StopBits, PL2303GMultiLib.Parity, PL2303GMultiLib.FlowControl) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Open an PL-UART USB Device by UART setting.
PL2303Read(int, byte[]) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Read Binary Data from PL2303G chip.
PL2303Release() - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Close an PL2303G USB Device.
PL2303SetupCOMPort(int, PL2303GMultiLib.BaudRate, PL2303GMultiLib.DataBits, PL2303GMultiLib.StopBits, PL2303GMultiLib.Parity, PL2303GMultiLib.FlowControl) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Setup basic communication parameters on PL2303G chip.
PL2303USBFeatureSupported() - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Detecting whether this Android OS supports USB host API feature.
PL2303Write(int, byte[]) - Method in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
  Writes n bytes Data to PL-UART chipset.
PLUART_DETACHED - Variable in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
PLUART_MESSAGE - Variable in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
Prolific_DevicePath_2_COMNumber - Variable in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib
ProlificUSBCurrentDeviceList - Variable in class tw.com.prolific.pl2303gmultilib.PL2303GMultiLib

B E P T V